- + 9123 456 7890
- info@goyalgroup.com

##### Billets

##### Our Products

- Sponge Iron
- Ferro Alloys
- Billets
- TMT Bars
- Wire Rod

##### Download

Company Presentation
Product Brochure

##### Contact Us

##### Billets

BDG Metal produces a wide range of continuously casted Billets in its Integrated Steel Plant. The state-of- art technology ensures international quality standards and ensures smooth and defect-free casting of billets. M.S. Billets are used for rolling of TMT Re-Bars of Fe 415/415D, Fe 500/500D, Fe 550/550D & Fe 600 Grade. The following are the specification of Billets available with BDG Metal & Power.

##### Physical Properties

DESCRIPTION | AS PER IS 2830 | BDG BILLETS
--- | --- | ---
Bend (max.) | 5 mm per meter | >= 5 mm per meter
Camber (max.) | 3mm per meter | >= 3 mm per meter
Length | 3 mt to 13 mt | 3 mt to 9 mt

##### Chemical Analysis as per BIS 2830 : 2012

DESIGNATION | %CARBON | %MANGANESE
--- | --- | ---
C15 | 0.12-0.18 + | 0.30-0.60
C18 | 0.15-0.21 | 0.30-0.60
C20 | 0.17-0.23 | 0.30-0.60
C15 MMn | 0.12-0.18 | 0.60-1.00
C18 MMn | 0.15-0.21 | 0.60-1.00
C20 MMn | 0.17-0.23 | 0.60-1.00
C15 HMn | 0.12-0.18 | 1.00-1.80
C18 HMn | 0.15-0.21 | 1.00-1.80
C20 HMn | 0.17-0.23 | 1.00-1.80

##### Chemical Analysis

GRADE | SULPHUR | PHOSPHOROUS | CARBON EQUIVALENT (CE)1
--- | --- | --- | ---
| Max | Max | Max
A | 0.050 | 0.050 | 0.42
B | 0.045 | 0.045 | 0.41
C | 0.040 | 0.040 | 0.39

##### Ferro Chrome

| SPECIFICATION (A) | SPECIFICATION (B) | SPECIFICATION (C)
--- | --- | --- | ---
Mn. | 58% - 60% Min | 60% Min | 60% Min
Si. | 3.5/4% Max | 3% Max | 2.5% Max
C. | 8% Max | 8% Max | 8/8.5% Max
S. | 0.05% Max | 0.05% Max | 0.05% Max
P. | 0.035% Max | 0.035% Max | 0.035% Max

##### ©2023 BDG Metal & Power Limited, All Rights Reserved.

- Home
- Site Map
- Terms and Conditions
- Privacy Policy