- Home
- Products
- Solar Mounting Structure

#### Overview

An experienced manufacturer of solar products & components. Ratan’s offers complete range of module mounting structures for PV based solar power and rooftop projects to suit ground or roof PV installations.

We can provide both hot dipped galvanization and pre-galvanized sheet structure. The structures are galvanized giving smooth and uniform thickness. The process is carried out under supervision of qualified engineers to ensure conformance to the following applicable standards.

##### Key Offerings

##### Design

##### Quality Assurance

##### Shop Assembly

##### Delivery at Site

##### Manufacture

##### Quality Control

##### Shop Testing

#### Ground Mounted Module Mounting Structure

Ground mounted structures consist of PV Modules (framed/unframed) held in place by racks or frames that are attached to the ground based mounting structure depending upon the nos. of modules per unit.

Every structure developed is a good bend of optimization and customization i.e. these structures can be customized to fit any type of PV module and can be optimized for varied soil types ranging from sandy deserts to hard rocky terrain. The arrangement of modules can either be Landscape or Portrait Oriented.

Ground Mounted Structure Variants : IS:2633 , IS:4759 , IS:6749

##### Ground Mounted Structure Supports

Foundation mounts-fixed to concrete slabs or poured footings

Ballasted footing mounts-concrete or steel bases that use weight to secure the solar panel system in position and do not require ground penetration. This type of mounting system is well suited for sites where excavation is not possible such as capped landfills. These systems simplify decommissioning or relocation of solar panel systems.

#### Roof Mounted Solar Structures

Roof mounted solar power systems consist of solar panels held in place by racks or frames attached to roof based mounting support.

##### Roof mounting structure supports

Pole Mounts attached directly to the roof structure and may use additional rails to hold the panel racking or frames.

##### Products

- Thickness: 0.6 mm to 8 mm
- Length: Upto 1200mm
- Material: CR Steel, HR Steel, Galvanized Steel, POSMAC
- Yield Strength: 245MPa to 345 MPa
- Type: Bare, Pre-galvanized and Hot dip galvanized
- Hot Dip Galvanization Thickness: 65 microns & above

##### Various Categories

- Ground Mounting Structure
- Rooftop Mounting Structure
- Carport Mounting Structure
- Solar Water Storage Mounting Structure

#### Industrial Applications

Ratan’s covers a wide range of structural requirements. Some of the technologies for which we offer our services includes:

- Fixed Angle / Rigid Model
- Tilting Mechanism
- Tracker Mechanism

Ratan’s caters Solar Module Mounting Structures of various categories
such as:

- Solar Parks
- Grid Connected Solar Projects
- Roof Top Solar Projects
- Captive Solar Power Plant

We supply structures to most EPC companies, Project Developers, Independent Power Producers, Captive Power units for Commercial & Industrial entities and several others.