- + 9123 456 7890
- info@goyalgroup.com

##### Ferro Alloys

##### Our Products

- Sponge Iron
- Ferror Alloys
- Billets
- TMT Bars
- Wire Rod

##### Download

Company Presentation
Product Brochure

##### Contact Us

##### Ferro Alloys

TFerro alloy refers to various alloys of iron with a highproportion of one or more other elements such as manganese,aluminium, or silicon. They are used in the production ofsteels and alloys.

##### Silico Manganese

| SPECIFICATION (A) GRADE:60/14 | SPECIFICATION (B) GRADE:65/15 | SPECIFICATION (C) GRADE:65/16
--- | --- | --- | ---
Mn. | 60% Min | 65% Min | 65% Min
Si. | 14% Min | 15% Min | 16% Min
C. | 2.50% Max | 2.25% Max | 2.00% Max
S. | 0.03% Max | 0.03% Max | 0.03% Max
P. | 0.30% Max | 0.25% Max | 0.25% Max

##### Ferro High Carbon Manganese

| SPECIFICATION (A) GRADE:75% | SPECIFICATION (B) GRADE:70%
--- | --- | ---
Mn. | 75% Min | 70% Min
Si. | 1.5% Max | 1.5% Max
C. | 6% - 8% Max | 8% Max
S. | 0.04% Max | 0.05% Max
P. | 0.20% - 0.25% Max | 0.30% Max

##### Ferro Silicon

| SPECIFICATION (A)
--- | ---
Si. | 72% Min
Ai. | 1.5% Max
P. | 0.05% Max
S. | 0.05% Max

##### Ferro Chrome

| SPECIFICATION (A) | SPECIFICATION (B) | SPECIFICATION (C)
--- | --- | --- | ---
Mn. | 58% - 60% Min | 60% Min | 60% Min
Si. | 3.5/4% Max | 3% Max | 2.5% Max
C. | 8% Max | 8% Max | 8/8.5% Max
S. | 0.05% Max | 0.05% Max | 0.05% Max
P. | 0.035% Max | 0.035% Max | 0.035% Max

##### ©2023 BDG Metal & Power Limited, All Rights Reserved.

- Home
- Site Map
- Terms and Conditions
- Privacy Policy