- Home
- Products
- Cable Trays & Accessories
- Cable Trays & Accessories

##### Cable Trays & Accessories

Cable Trays Accessories include Horizontal & Vertical Bends, Reducers, Cross, Tees, Clamps, Slotted Angles, Flexible Jumpers, Coupler Plates etc. for Trays.

- ##### Material : MS Sheet & Angle / SS Sheet/ Aluminium Sheet & Angle etc.

- ##### Finish : Red Oxide/ Enamel Paint/ Epoxy Paint/ Powder Coating / Hot Dip Galvanised / Anodised or as per customer specification. H = 50 to 200 mm W/WW = 100 to 1200 mm D = 30/45/60/90/120 Deg R = 150 to 1200 mm Accessories can be made as per customer specification too.

##### Schedule of Permissible Loads

All figures given repressent the maximum permissible uniformly distributed load in kgs. per running
meter Unsupported Free Span

- ##### - Formula : The maximum permissible The maximum permissible point load at-mid-span may be
  obtained from the formula

- P = ½ X U X C
- Where P = maximum permissible point load in kgs at mid-span.
- U = maximum permissible uniformly distributed load in kg per running meter.
- S = the particular free span in meter